2023-09-05 星期二 10:20:20

设备体积小、易安装:产品尺寸仅与智能手机大小相当，具备积水探测、无线通讯、电源管理、智能控制等多个功能，产品安装运维无需土建施工，适用于道路、涵隧、地铁站等多种场景的内涝积水监测。
The equipment is small in size and easy to install: the product size is only about the size of a smart phone, andit has multiple functions such as water detection wireless communication, power management, and intel-ligent control: Productinstallatian and operation andmaintenance da not require civil construction, and aresuitable for waterlogging monitoring in various scenariossuch as roads,culverts and tunnels, and subway stations.

设备融合多种水深传感器和滤波算法，5米量程范围内精度可达1cm;采用多模多信道通信技术，业务响应毫秒级可达，核心部件实现全国产化，支持IPV6网络，性能稳定可靠。
The equipment integrates a variety of water depthsensors and filtering algorithms, and the accuracy canreach icm in the range of 5 meters; Using multi-mode andmulti-channelcommunication technology. serwiceresponse can reach milliseconds.The core componentshave been produced nationwide, support IPy6 networksand have stable and reliable performance.

设备应用了自主研发的自动分频上报算法和电源管理系统，可根据采集水深和电压智能识别内涝风险等级和预警上报频次，设备单次工作时间长达一年以上，可实现区域内涝联动预警。
The equipment applies the self-developed automatic frequency division reporting algorithm and power management system, which can intelligently identify thewaterlogging risk level and early warning reporting fre-quency according to the collected water depth andvoltage, and the equipment can work for more than one year at a time, which can realize the linkage early warningof waterlogging in the region.
水尺水深(Depth)【1#】: cm
水尺水深(Depth)【2#】: cm
TimeSelect: to ; DevSelect: